'components to exclude from full layer SM clearance grouping
'list part numbers, 1 per line, no spaces, no tab characters

<parts_to_exclude_from_sm_grouping>
M2P5_MNT_HOLE_236_PAD_VIAS
</parts_to_exclude_from_sm_grouping>



'the following variable / value pairs must be separated by a tab character.  

default_oversize_value	5
default_conductive_area_clearance	15

'options for units are: th, in, mm, um
oversize_value_unit	th
conductive_area_clearance_unit	th