'Notes: 
'each line in this file is composed of a key and a value, separated by a tab character
'the post processing software reads each line and uses the tab to separate the key from the value
'the values can be manually edited to produce different results in the output.
'where the key is repeated on several lines, a drop-down list is created in the software. 
'items can be added to the list by adding a new line with the same key, tab, and value syntax

copper_layer_thickness	
copper_layer_thickness	1/8 oz
copper_layer_thickness	1/4 oz
copper_layer_thickness	1/2 oz
copper_layer_thickness	1 oz
copper_layer_thickness	1 1/2 oz
copper_layer_thickness	2 oz
copper_layer_thickness	3 oz
copper_layer_thickness	4 oz
copper_layer_thickness	See Stackup Detail

board_thickness	.031
board_thickness	.040
board_thickness	.062
board_thickness	.070
board_thickness	.080
board_thickness	.090
board_thickness	.100
board_thickness	.110
board_thickness	.120
board_thickness	.125
board_thickness	.130
board_thickness	.140
board_thickness	.150

shipping_method	UPS Red
shipping_method	UPS Blue
shipping_method	UPS Ground
shipping_method	FedEx

etch_tolerance	Standard
etch_tolerance	.002
etch_tolerance	.004

depanel_method	Routed
depanel_method	Scored
depanel_method	Routed & Scored
depanel_method	None

board_material	FR-4
board_material	FR408
board_material	FR408HR
board_material	370HR
board_material	370
board_material	Polyimide
board_material	Teflon
board_material	Isola Itera MT

teflon_material	Cuclad 250
teflon_material	Rogers 3003

soldermask_material	LPI
soldermask_material	Epoxy
soldermask_material	SR1000
soldermask_material	Dry Film
soldermask_material	None

soldermask_sides	Top Side Only
soldermask_sides	Bottom Side Only
soldermask_sides	Both Sides
soldermask_sides	None

'template_url	http://home.aeroflex.com/ISO/ENG/FORMS/CURRENT/FRM50017I%20PCB%20Characterization.dot
template_url	X:\ENG\LIBRARY\RELEASED\Mentor\Templates and Support Files\FRM50017J_PCB_CHARACTERIZATION.docx

control_object_names
txt_cc1
cbo_depanel_method
cbo_pcb_thickness
cbo_cu_thk_inner
cbo_cu_thk_outer
cbo_cu_thk_all
cbo_board_material
cbo_etch_tolerance
txt_special_feature_tolerance
chk_special_feature_tolerance
txt_smallest_space
txt_smallest_trace
chk_smt
chk_tdr_testing
cbo_soldermask_type
txt_special_comments
chk_via_fill
chk_gold_edge
chk_silkscreen
chk_controlled_impedance
chk_continuity_test
rb_sm_over_enig
chk_soldermask
rb_sm_over_traces_with_enig
rb_smobc
txt_gold_edge_length
txt_gold_edge_width
/control_object_names

